Quotation No: QA 0504-6669_FCP - IO                             
Scout No:
Please refer to this number when ordering.

Date: 12/12/2011	
To:

Attn:
Email:
Tel:
Fax:	Tmwrf-Warehouse                    
8500 Clean Water Way               
Reno                                 NV   89502         
US 
MARK BOWMAN 

	Please send your purchase order to:
Invensys Systems USA
 6950 SW Hampton
 Suite 242
 Tigard,  OR  97223    
USA

Tel: 503 620-1743
Fax: 503 218-5700 
Email; Doug.Karleskint@Invensys.com

Inquiry Reference:    
Customer RFQ #:   

Please find attached quotation for the items you requested.
Orders placed on or before the expiration date will be billed at prices quoted.
This quote is valid for 30 from the date of this quote. 

Firm Prices: Prices are in US Dollars and are firm for all Invensys IOM equipment shipped and/or services. Pricing level is for a single purchase order. Multiple purchase orders may affect pricing.

Taxes and Duties: Sales taxes, duties and other fees are not included in this quotation.

All invoices are due and payable within 30 days from invoice date. Late charges may result in a late payment fee.

Freight: FOB, Foxboro MA

Estimated Shipment: 4 to 6 Weeks

Travel and Living expenses (if applicable) are in addition at cost plus 10%	
Notes: 

Doug Karleskint                         

  Item 	Qty 	Model 	Description 	
    20.00 	 1 	 P0926HC 	 2 FCP Slots Hor. Baseplate, Time Strobe 	 
    	  	 PSS Reference:  21H-2W6 B4   	 
  P0926HC   	 FUNCTION: 2 FCP Slots Hor. Baseplate, Time Strobe Horizontal Baseplate For A Fault-Tolerant FCP270 With Time Strobe And Local Fieldbus Connectors. 	  	 

  Item 	Qty 	Model 	Description 	
    20.01 	 1 	 P0916MZ 	 2 Mbps Base To Base Cable, 1m 	 
    	  	 PSS Reference:  21H-2X2 B4   	 
  P0916MZ   	 FUNCTION: 2 Mbps Base To Base Cable, 1m Cable To Connect 2 Mbps Module Fieldbus Between P0940XA Or P0940XB Baseplates.  One Cable Provides Bus Redundancy. 	  	 

  Item 	Qty 	Model 	Description 	
    20.02 	 2 	 P0926KN 	 Power Supply Output Cable - 152 cm (60 in) 	 
   P0926KN   	 FUNCTION: Power Supply Output Cable - 152 cm (60 in) Cable To Connect P0917LY Power Supply To Modular Baseplate.  One Cable Per Baseplate Required For Non-Redundant Power, Two Cables For Redundant Cable.  Length 60 Inches / 152 cm. 	  	 

  Item 	Qty 	Model 	Description 	
    30.00 	 4 	 P0916RB 	 Fieldbus Baseplate Terminator 	 
    	  	 PSS Reference:  21H-2X2 B4   	 
  P0916RB   	 FUNCTION: Fieldbus Baseplate Terminator Connector With Termination Resistors.  Plugs Into A Connector On The Baseplate.  Two Are Required For Each Module Fieldbus Branch Consisting Of 1 To 4 Baseplates. 	  	 

  Item 	Qty 	Model 	Description 	
    40.00 	 2 	 P0926HT 	 8 Slots Hor. Baseplate, Time Strobe, 8FBM 	 
    	  	 PSS Reference:  21H-2W6 B4   	 
  P0926HT   	 FUNCTION: 8 Slots Hor. Baseplate, Time Strobe, 8FBM Horizontal Baseplate With 8 FBMs' Slots, With Time Strobe And Local Fieldbus Connectors. 	  	 

  Item 	Qty 	Model 	Description 	
    40.01 	 1 	 P0916NA 	 2 Mbps Base To Base Cable, 10m 	 
    	  	 PSS Reference:  21H-2X2 B4   	 
  P0916NA   	 FUNCTION: 2 Mbps Base To Base Cable, 10m Cable To Connect 2 Mbps Module Fieldbus Between P0940XA Or P0940XB Baseplates.  One Cable Provides Bus Redundancy. 	  	 

  Item 	Qty 	Model 	Description 	
    40.02 	 4 	 P0926KM 	 Power Supply Output Cable - 121 cm (48 in) 	 
   P0926KM   	 FUNCTION: Power Supply Output Cable - 121 cm (48 in) Cable To Connect P0917LY Power Supply To Modular Baseplate.  One Cable Per Baseplate Required For Non-Redundant Power, Two Cables For Redundant Cable.  Length 48 Inches / 121 cm. 	  	 

  Item 	Qty 	Model 	Description 	
    50.00 	 4 	 P0922YU 	 Power Supply, FPS 400-24 	 
    	  	 PSS Reference:  21H-2W3 B4   	 
  P0922YU   	 FUNCTION: Power Supply, FPS 400-24 Power Supply With Universal ac/dc Mains @ 85/265 Vac 47/63 Cycles Or 125 Vdc; Output 24 Vdc.  UL And UL-C Listed For Class I, Division 2, Groups A,B,C,D And CENELEC Certified For Zone 2 Group IIC.  For G3 Environmental Locations.  Rated Output 400 Watts. 	  	 

  Item 	Qty 	Model 	Description 	
    50.01 	 4 	 P0926TM 	 110/240V FPS Power Cable, 4 Ft 	 
    	  	 PSS Reference:  21H-2W3 B4   	 
  P0926TM   	 FUNCTION: 110/240V FPS Power Cable, 4 Ft Cable to connect input power connection kit to P0922YU power supply.   One cable per power supply required.  Length 4 feet. 	  	 

  Item 	Qty 	Model 	Description 	
    50.02 	 4 	 P0926DZ 	 Power Connection Kit For FPS 400-24 	 
    	  	 PSS Reference:  21H-2W3 B4   	 
  P0926DZ   	 FUNCTION: Power Connection Kit For FPS 400-24 Input Power Connection Kit For FPS 400-24.  Includes Terminal Blocks. 	  	 

  Item 	Qty 	Model 	Description 	
    60.00 	 1 	 P0914SQ 	 FBM201 Channel Isolated 8 Input 0-20 mA 	 
    	  	 PSS Reference:  21H-2Z1 B4   	 
  P0914SQ   	 FUNCTION: FBM201 Channel Isolated 8 Input 0-20 mA FBM Module For Mounting On DIN Rail Baseplate. Provides Per Channel Loop Power With Per Channel Isolation.  Termination Assembly Allows Per Channel Selection For FBM Loop Power Or External Power. 	  	 

  Item 	Qty 	Model 	Description 	
    60.01 	 1 	 P0916AA 	 Compression Term Assembly, FBM201 	 
    	  	 PSS Reference:  21H-2Z1 B4   	 
  P0916AA   	 FUNCTION: Compression Term Assembly, FBM201 Three Tier Compression Style Term Block for FBM Powered Or External Powered Loops. 	  	 

  Item 	Qty 	Model 	Description 	
    60.02 	 1 	 P0916DB 	 FBM2xx Type 1 Term Cable, 1 Meter 	 
    	  	 PSS Reference:  21H-2W1 B3   	 
  P0916DB   	 FUNCTION: FBM2xx Type 1 Term Cable, 1 Meter 8 Channel Triad Termination Cable, 37Dsub to 25Dsub for use on Channel Isolated FBMs Type 201, 203, 204, 205, 206, 237.  Shielded cable polyurethane outer jacket, PVC insulation on inner wires. 	  	 

  Item 	Qty 	Model 	Description 	
    70.00 	 1 	 P0914SY 	 FBM204 4 Channel 0-20 In + 4 Channel 0-20 Out 	 
    	  	 PSS Reference:  21H-2Z4 B4   	 
  P0914SY   	 FUNCTION: FBM204 4 Channel 0-20 In + 4 Channel 0-20 Out FBM Module For Mounting On DIN Rail Baseplate. Provides Per Channel Loop Power With Per Channel Isolation. 	  	 

  Item 	Qty 	Model 	Description 	
    70.01 	 1 	 P0916AG 	 Compression Term Assembly, FBM204 	 
    	  	 PSS Reference:  21H-2Z4 B4   	 
  P0916AG   	 FUNCTION: Compression Term Assembly, FBM204 Three Tier Compression Style Term Block For FBM Powered Or External Powered Loops. 	  	 

  Item 	Qty 	Model 	Description 	
    70.02 	 1 	 P0916DB 	 FBM2xx Type 1 Term Cable, 1 Meter 	 
    	  	 PSS Reference:  21H-2W1 B3   	 
  P0916DB   	 FUNCTION: FBM2xx Type 1 Term Cable, 1 Meter 8 Channel Triad Termination Cable, 37Dsub to 25Dsub for use on Channel Isolated FBMs Type 201, 203, 204, 205, 206, 237.  Shielded cable polyurethane outer jacket, PVC insulation on inner wires. 	  	 

  Item 	Qty 	Model 	Description 	
    80.00 	 2 	 P0916RH 	 FBM219, Discrete I/O, 32 Channels, 24 DIN+8 DOUT 	 
    	  	 PSS Reference:  21H-2Z19 B4   	 
  P0916RH   	 FUNCTION: FBM219, Discrete I/O, 32 Channels, 24 DIN+8 DOUT FBM219 Provides 24 Two Wire Input Channels For Monitoring On/Off Voltage Levels And 8 Two Wires Channels For Externally Sourced Outputs.  Termination Assemblies Are Available To Support A Variety Of Discrete Signal Types And Voltage Ranges. 	  	 

  Item 	Qty 	Model 	Description 	
    80.01 	 2 	 P0917LS 	 Comp TA FBM219 125V Switch DI + 5A Relay Out 	 
    	  	 PSS Reference:  21H-2Z19 B4   	 
  P0917LS   	 FUNCTION: Comp TA FBM219 125V Switch DI + 5A Relay Out Two/Three Tier Compression Style Term Block For Connection Of 24 DI Circuits In Configuration For Switch Type DI With Two Pairs For Distribution Of 120 Vac/125 Vdc Wetting Voltage, Plus 8 DO Circuits Using 5A Form C Relay For Applications With External Fusing And Power Distribution. 	  	 

  Item 	Qty 	Model 	Description 	
    80.02 	 2 	 P0916FH 	 FBM2xx Type 4 Term Cable, 1 Meter 	 
    	  	 PSS Reference:  21H-2W1 B3   	 
  P0916FH   	 FUNCTION: FBM2xx Type 4 Term Cable, 1 Meter 18 Twisted Pair 26 AWG Termination Cable, 37Dsub To 37Dsub For Use On 16 Channel Differential Input FBMs, Discrete FBMs, And 32 Channel Group Discrete Types 207, 207b, 207c, 211, 212, 217, 219, 241, 241b, 241c, 241d, 242.  Shielded Cable, Polyurethane Outer Jacket, PVC Insulation On Inner Wires. 	  	 

  Item 	Qty 	Model 	Description 	
    90.00 	 5 	 P0914TD 	 FBM207 Channel Isolated 16 DIN Voltage Monitor 	 
    	  	 PSS Reference:  21H-2Z7 B4   	 
  P0914TD   	 FUNCTION: FBM207 Channel Isolated 16 DIN Voltage Monitor FBM Module For Mounting On DIN Rail Baseplate. Provides 16 Isolated Channels For Monitoring On/Off Voltage Levels.  Term Assemblies Available For Voltage Monitoring Inputs Of 15-60 Vdc, 120 Vac/125 Vdc, And 240 Vac; Or Switch Inputs With 120 Vac/125 Vdc, Or 240 Vac Excitation. 	  	 

  Item 	Qty 	Model 	Description 	
    90.01 	 5 	 P0916PK 	 Compression Term Assy, FBM207, 120/125V Switch DI 	 
    	  	 PSS Reference:  21H-2Z7 B4   	 
  P0916PK   	 FUNCTION: Compression Term Assy, FBM207, 120/125V Switch DI Two Tier Compression Style Term Block For Connection Of 16 DI Circuits In Configuration For Switch Type Digital Inputs.  Term Assembly Contains Conditioning Circuits For 120 Vac/125 Vdc Circuits Plus A Two Pair Terminal Block With Fuse For Distributing The 120/125 Wetting Voltage To The Switch Inputs. 	  	 

  Item 	Qty 	Model 	Description 	
    90.02 	 5 	 P0916FH 	 FBM2xx Type 4 Term Cable, 1 Meter 	 
    	  	 PSS Reference:  21H-2W1 B3   	 
  P0916FH   	 FUNCTION: FBM2xx Type 4 Term Cable, 1 Meter 18 Twisted Pair 26 AWG Termination Cable, 37Dsub To 37Dsub For Use On 16 Channel Differential Input FBMs, Discrete FBMs, And 32 Channel Group Discrete Types 207, 207b, 207c, 211, 212, 217, 219, 241, 241b, 241c, 241d, 242.  Shielded Cable, Polyurethane Outer Jacket, PVC Insulation On Inner Wires. 	  	 

  Item 	Qty 	Model 	Description 	
    100.00 	 2 	 P270001010M0 	 Advantage Upgrade from older CPs to CP270 	 
    	  	 PSS Reference:  21H-1B9 B3   	 
  P270   	 FUNCTION: Paper document that identifies children FCP270 (P0917YZ) Baseplate Mounted Control Processor Or ZCP270 (P0926CP) Control Processor Implemented In A "Z" Form Factor. Both With Control Network And Fieldbus Network Connections Using 100 Mbps Fiber Optic.     	  	 
   0   	 I/A SERIES VERSION: For Version 8.x System  	  	 
   0   	 CONTROLLER TYPE: FCP270 Control Processor  	  	 
   1   	 FUTURE OPTION: Not used  	  	 
   0   	 FUTURE OPTION: Not used  	  	 
   1   	 FUTURE OPTION: Not used  	  	 
   0   	 FUTURE OPTION: Not used  	  	 
   M   	 HARDWARE TRADE-IN UPGRADE CREDIT: SvcAgmt Adv Discount for MicroIA Return  	  	 
   0   	 ADDITIONAL DISCOUNT FOR RETURN OF ADDITIONAL PRODU No return  	  	 

  Item 	Qty 	Model 	Description 	
    100.01 	 2 	 P0917YZ 	 FCP270 Control Processor 	 
    	  	 PSS Reference:  21H-1B9 B3   	 
  P0917YZ   	 FUNCTION: FCP270 Control Processor Baseplate Mounted Control Processor.  Control Network And Fieldbus Network Connections Are 100 Mbps Fiber Optic 	  	 

  Item 	Qty 	Model 	Description 	
    100.02 	 2 	 P0973BU 	 0.25 m LC-LC Fiber Optic Jumper Cable, Gray 	 
    	  	 PSS Reference:  21H-2W6 B4   	 
  P0973BU   	 FUNCTION: 0.25 m LC-LC Fiber Optic Jumper Cable, Gray Fiber Optic Cable using LC connections.  Intended for use with FCP270 connections to splitter combiners. 	  	 

  Item 	Qty 	Model 	Description 	
    100.03 	 2 	 P0972ZQ 	 0.25 m LC-LC Fiber Optic Jumper Cable, Orange 	 
   P0972ZQ   	 FUNCTION: 0.25 m LC-LC Fiber Optic Jumper Cable, Orange Fiber Optic Cable Using LC Connections Intended For Use With FCP270 Connections To Splitter Combiners. 	  	 

  Item 	Qty 	Model 	Description 	
    100.04 	 1 	 P0926MX 	 Splitter / Combiner Kit (With 2 Modules) 	 
   P0926MX   	 FUNCTION: Splitter / Combiner Kit (With 2 Modules) Splitter Combiner Kit Which Includes 2 Splitter/Combiners, Bracket And Hardware 	  	 

  Item 	Qty 	Model 	Description 	
    100.05 	 2 	 P0972TS 	 15 m MMF, Fiber, MT-RJ To LC Adapter Cable 	 
   P0972TS   	 FUNCTION: 15 m MMF, Fiber, MT-RJ To LC Adapter Cable 15 Meter Fiber, MMF, 62.5/125 um, Plenum, MT-RJ To LC Adapter Cable Used To Connect FCP/ZCPs To MT-RJ Fiber Switches.  Has PVC Content. 	  	 

  Item 	Qty 	Model 	Description 	
    150.00 	 1 	 S61C1121100X 	 I/A Series Function Block SW Lic (Certificate) 	 
   S61   	 FUNCTION: I/A Series Software License Entitling User To Use The Specified I/A Series Function Block Software Selections. Paper license certificate. 	  	 
   C   	 VERSION: For Use On FCP270, ZCP270, Triconex or Gateway FBM  	  	 
   1   	 ANALOG INPUT QTY: Up To 50 Analog Inputs  	  	 
   1   	 ANALOG OUTPUT QTY: Up To 50 Analog Outputs  	  	 
   2   	 DIGITAL INPUT QTY: Up To 100 Digital Inputs  	  	 
   1   	 DIGITAL OUTPUT QTY: Up To 50 Digital Outputs  	  	 
   1   	 LICENSE TYPE: Fault Tolerant Control & Monitoring  	  	 
   0   	 FUTURE OPTION: Not Used  	  	 
   0   	 FUTURE OPTION: Not Used  	  	 
   X   	 UPGRADES: SvcAgmt Adv Discount for MicroIA Return  	  	 
   Tags  	
Set 1 	 1 	 Customer Name 	 CITY OF SPARKS 	
	 1 	 Customer Site 	 SPARKS 	
	 1 	 Process Cell Name 	 S61License2 	

  Item 	Qty 	Model 	Description 	
    160.00 	 1 	 VAS-S-IA-AP 	 Advantage Program Services-IA 	 
   VAS-S-IA-AP   	 FUNCTION: Advantage Program Services-IA Field Service technical review of Advantage quotation and site survey to ensure consistency with customer requirements. Includes installation and startup services. 	  	 
  
    Quote Sell List: 	$47,363.85 	Quote Sell Net: 	$29,330.14